038e58a2: ndt_2c Msg: Querying if test miniport is wireless
038e58a2: ndt_2c Msg: Miniport AX88772b1 is ** NOT Wireless-LAN **
<TESTGROUP>

*** ==================================================================
*** SUITE INFORMATION
***
*** Suite Name:        N/A (built on the fly)
*** Suite Description: N/A
*** Number of Tests:   6
*** ==================================================================

*** ==================================================================
*** SYSTEM INFORMATION
***
*** Date and Time:          11/16/2011 10:55 PM (Wednesday)
***
*** Device Name:            CEPC
***
*** OS Version:             5.0
*** Build Number:           1400
*** Platform ID:            3 "Windows CE"
*** Version String:         ""
***
*** Processor Type:         0x000002AE (686) "Intel Pentium II"
*** Processor Architecture: 0x0000     (0) "Intel"
*** Page Size:              0x00001000 (4,096)
*** Minimum App Address:    0x00010000 (65,536)
*** Maximum App Address:    0x7FFFFFFF (2,147,483,647)
*** Active Processor Mask:  0x00000001
*** Number Of Processors:   1
*** Allocation Granularity: 0x00010000 (65,536)
*** Processor Level:        0x0002     (2)
*** Processor Revision:     0x0004     (4)
*** ==================================================================

*** ==================================================================
*** MEMORY INFO
***
*** Memory Total:    24,485,888 bytes
*** Memory Used:     11,026,432 bytes
*** Memory Free:     13,459,456 bytes
***
*** Kernel Used:        937,984 bytes
*** Water Mark:           3,283 pages
***
*** Store Total:     24,416,256 bytes
*** Store Used:         601,904 bytes
*** Store Free:      23,814,352 bytes
*** ==================================================================

BEGIN GROUP: ndt_2c.dll
<TESTCASE ID=1>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      2c_SendPackets
*** Test ID:        1
*** Library Path:   \ndt_2c.dll
*** Command Line:   -t AX88772b1 -s AX88772b1
*** Random Seed:    5424
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "2c_SendPackets", Threads=0, Seed=5424
      038e58a2: ndt_2c Msg: Start 2c_SendPackets test
      038e58a2: ndt_2c Msg: The test adapter is AX88772b1
      038e58a2: ndt_2c Msg: The support adapter is AX88772b1
      038e58a2: ndt_2c Msg: Opening adapters
      038e58a2: ndt_2c Msg: Binding adapters
      038e58a2: ndt_2c Msg: Get basic adapters info
      038e58a2: ndt_2c Msg: Set adapter filters
      038e58a2: ndt_2c Msg: Sending 300 packets with size 64 bytes to 1 addresses
      038e58a2: ndt_2c Msg: Sent 300 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 300 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 783 bytes to 1 addresses
      038e58a2: ndt_2c Msg: Sent 300 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 300 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 1500 bytes to 1 addresses
      038e58a2: ndt_2c Msg: Sent 300 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 300 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 64 bytes to 2 addresses
      038e58a2: ndt_2c Msg: Sent 600 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 600 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 783 bytes to 2 addresses
      038e58a2: ndt_2c Msg: Sent 600 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 600 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 1500 bytes to 2 addresses
      038e58a2: ndt_2c Msg: Sent 600 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 600 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 64 bytes to 3 addresses
      038e58a2: ndt_2c Msg: Sent 900 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 900 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 783 bytes to 3 addresses
      038e58a2: ndt_2c Msg: Sent 900 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 900 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 1500 bytes to 3 addresses
      038e58a2: ndt_2c Msg: Sent 900 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 900 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 64 bytes to 4 addresses
      038e58a2: ndt_2c Msg: Sent 1200 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 1200 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 783 bytes to 4 addresses
      038e58a2: ndt_2c Msg: Sent 1200 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 1200 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 1500 bytes to 4 addresses
      038e58a2: ndt_2c Msg: Sent 1200 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 1200 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 64 bytes to 5 addresses
      038e58a2: ndt_2c Msg: Sent 1500 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 1500 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 783 bytes to 5 addresses
      038e58a2: ndt_2c Msg: Sent 1500 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 1500 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 1500 bytes to 5 addresses
      038e58a2: ndt_2c Msg: Sent 1500 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 1500 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 64 bytes to 6 addresses
      038e58a2: ndt_2c Msg: Sent 1800 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 1800 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 783 bytes to 6 addresses
      038e58a2: ndt_2c Msg: Sent 1800 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 1800 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 1500 bytes to 6 addresses
      038e58a2: ndt_2c Msg: Sent 1800 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 1800 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 64 bytes to 7 addresses
      038e58a2: ndt_2c Msg: Sent 2100 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 2100 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 783 bytes to 7 addresses
      038e58a2: ndt_2c Msg: Sent 2100 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 2100 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 1500 bytes to 7 addresses
      038e58a2: ndt_2c Msg: Sent 2100 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 2100 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 64 bytes to 8 addresses
      038e58a2: ndt_2c Msg: Sent 2400 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 2400 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 783 bytes to 8 addresses
      038e58a2: ndt_2c Msg: Sent 2400 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 2400 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 1500 bytes to 8 addresses
      038e58a2: ndt_2c Msg: Sent 2400 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 2400 packets
      038e58a2: ndt_2c Msg: Unbinding adapters
   END TEST: "2c_SendPackets", PASSED, Time=339.150
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      2c_SendPackets
*** Test ID:        1
*** Library Path:   \ndt_2c.dll
*** Command Line:   -t AX88772b1 -s AX88772b1
*** Result:         Passed
*** Random Seed:    5424
*** Thread Count:   1
*** Execution Time: 0:05:39.150
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=2>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      2c_ReceivePackets
*** Test ID:        2
*** Library Path:   \ndt_2c.dll
*** Command Line:   -t AX88772b1 -s AX88772b1
*** Random Seed:    17751
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "2c_ReceivePackets", Threads=0, Seed=17751
      038e58a2: ndt_2c Msg: Start 2c_ReceivePackets test
      038e58a2: ndt_2c Msg: The test adapter is AX88772b1
      038e58a2: ndt_2c Msg: The support adapter is AX88772b1
      038e58a2: ndt_2c Msg: Opening adapters
      038e58a2: ndt_2c Msg: Binding adapters
      038e58a2: ndt_2c Msg: Get basic adapters info
      038e58a2: ndt_2c Msg: Set adapter filters
      038e58a2: ndt_2c Msg: Sending 300 packets with size 64 bytes to 8 addresses
      038e58a2: ndt_2c Msg: Sent 2400 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 2400 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 783 bytes to 8 addresses
      038e58a2: ndt_2c Msg: Sent 2400 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 2400 packets
      038e58a2: ndt_2c Msg: Sending 300 packets with size 1500 bytes to 8 addresses
      038e58a2: ndt_2c Msg: Sent 2400 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Received 2400 packets
      038e58a2: ndt_2c Msg: Unbinding adapters
   END TEST: "2c_ReceivePackets", PASSED, Time=42.508
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      2c_ReceivePackets
*** Test ID:        2
*** Library Path:   \ndt_2c.dll
*** Command Line:   -t AX88772b1 -s AX88772b1
*** Result:         Passed
*** Random Seed:    17751
*** Thread Count:   1
*** Execution Time: 0:00:42.508
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=3>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      2c_FilterReceive
*** Test ID:        3
*** Library Path:   \ndt_2c.dll
*** Command Line:   -t AX88772b1 -s AX88772b1
*** Random Seed:    25237
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "2c_FilterReceive", Threads=0, Seed=25237
      038e58a2: ndt_2c Msg: Start 2c_FilterReceive test
      038e58a2: ndt_2c Msg: The test adapter is AX88772b1
      038e58a2: ndt_2c Msg: The support adapter is AX88772b1
      038e58a2: ndt_2c Msg: Opening adapters
      038e58a2: ndt_2c Msg: Binding adapters
      038e58a2: ndt_2c Msg: Get basic adapters info
      038e58a2: ndt_2c Msg: Possible filter settings:
      038e58a2: ndt_2c Msg:   - Directed
      038e58a2: ndt_2c Msg:   - Broadcast
      038e58a2: ndt_2c Msg:   - Promiscuous
      038e58a2: ndt_2c Msg:   - Multicast
      038e58a2: ndt_2c Msg:   - All Multicast
      038e58a2: ndt_2c Msg: Setting receiving filters
      038e58a2: ndt_2c Msg: Set filter FILTER_NONE for instance 0
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+ for instance 1
      038e58a2: ndt_2c Msg: Set filter FILTER_BROADCAST+ for instance 2
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      038e58a2: ndt_2c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      038e58a2: ndt_2c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      038e58a2: ndt_2c Msg: Start receiving
      038e58a2: ndt_2c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Instance 0 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 1 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 2 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 3 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 4 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 5 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 6 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 7 received expected 300 packets
      038e58a2: ndt_2c Msg: Setting receiving filters
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+ for instance 0
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      038e58a2: ndt_2c Msg: Start receiving
      038e58a2: ndt_2c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Instance 0 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 1 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 2 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 3 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 4 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 5 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 6 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 7 received expected 300 packets
      038e58a2: ndt_2c Msg: Setting receiving filters
      038e58a2: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      038e58a2: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      038e58a2: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      038e58a2: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      038e58a2: ndt_2c Msg: Start receiving
      038e58a2: ndt_2c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Instance 0 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 1 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 2 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 3 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 4 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 5 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 6 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 7 received expected 300 packets
      038e58a2: ndt_2c Msg: Setting receiving filters
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      038e58a2: ndt_2c Msg: Start receiving
      038e58a2: ndt_2c Msg: Sending 300 packets with size 128 bytes to Test NIC's directed Addr
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Instance 0 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 1 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 2 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 3 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 4 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 5 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 6 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 7 received expected 300 packets
      038e58a2: ndt_2c Msg: Setting receiving filters
      038e58a2: ndt_2c Msg: Set filter FILTER_NONE for instance 0
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+ for instance 1
      038e58a2: ndt_2c Msg: Set filter FILTER_BROADCAST+ for instance 2
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      038e58a2: ndt_2c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      038e58a2: ndt_2c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      038e58a2: ndt_2c Msg: Start receiving
      038e58a2: ndt_2c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Instance 0 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 1 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 2 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 3 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 4 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 5 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 6 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 7 received expected 300 packets
      038e58a2: ndt_2c Msg: Setting receiving filters
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+ for instance 0
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      038e58a2: ndt_2c Msg: Start receiving
      038e58a2: ndt_2c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Instance 0 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 1 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 2 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 3 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 4 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 5 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 6 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 7 received expected 300 packets
      038e58a2: ndt_2c Msg: Setting receiving filters
      038e58a2: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      038e58a2: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      038e58a2: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      038e58a2: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      038e58a2: ndt_2c Msg: Start receiving
      038e58a2: ndt_2c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Instance 0 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 1 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 2 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 3 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 4 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 5 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 6 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 7 received expected 300 packets
      038e58a2: ndt_2c Msg: Setting receiving filters
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      038e58a2: ndt_2c Msg: Start receiving
      038e58a2: ndt_2c Msg: Sending 300 packets with size 128 bytes to Broadcast Addr
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Instance 0 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 1 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 2 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 3 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 4 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 5 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 6 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 7 received expected 300 packets
      038e58a2: ndt_2c Msg: Setting receiving filters
      038e58a2: ndt_2c Msg: Set filter FILTER_NONE for instance 0
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+ for instance 1
      038e58a2: ndt_2c Msg: Set filter FILTER_BROADCAST+ for instance 2
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      038e58a2: ndt_2c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      038e58a2: ndt_2c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      038e58a2: ndt_2c Msg: Start receiving
      038e58a2: ndt_2c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Instance 0 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 1 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 2 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 3 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 4 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 5 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 6 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 7 received expected 300 packets
      038e58a2: ndt_2c Msg: Setting receiving filters
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+ for instance 0
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      038e58a2: ndt_2c Msg: Start receiving
      038e58a2: ndt_2c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Instance 0 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 1 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 2 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 3 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 4 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 5 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 6 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 7 received expected 300 packets
      038e58a2: ndt_2c Msg: Setting receiving filters
      038e58a2: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      038e58a2: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      038e58a2: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      038e58a2: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      038e58a2: ndt_2c Msg: Start receiving
      038e58a2: ndt_2c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Instance 0 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 1 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 2 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 3 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 4 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 5 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 6 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 7 received expected 300 packets
      038e58a2: ndt_2c Msg: Setting receiving filters
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      038e58a2: ndt_2c Msg: Start receiving
      038e58a2: ndt_2c Msg: Sending 300 packets with size 128 bytes to Any directed Random Addr
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Instance 0 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 1 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 2 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 3 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 4 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 5 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 6 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 7 received expected 300 packets
      038e58a2: ndt_2c Msg: Setting receiving filters
      038e58a2: ndt_2c Msg: Set filter FILTER_NONE for instance 0
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+ for instance 1
      038e58a2: ndt_2c Msg: Set filter FILTER_BROADCAST+ for instance 2
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      038e58a2: ndt_2c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      038e58a2: ndt_2c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      038e58a2: ndt_2c Msg: Start receiving
      038e58a2: ndt_2c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Instance 0 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 1 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 2 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 3 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 4 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 5 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 6 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 7 received expected 300 packets
      038e58a2: ndt_2c Msg: Setting receiving filters
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+ for instance 0
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      038e58a2: ndt_2c Msg: Start receiving
      038e58a2: ndt_2c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Instance 0 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 1 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 2 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 3 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 4 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 5 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 6 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 7 received expected 300 packets
      038e58a2: ndt_2c Msg: Setting receiving filters
      038e58a2: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      038e58a2: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      038e58a2: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      038e58a2: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      038e58a2: ndt_2c Msg: Start receiving
      038e58a2: ndt_2c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Instance 0 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 1 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 2 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 3 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 4 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 5 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 6 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 7 received expected 300 packets
      038e58a2: ndt_2c Msg: Setting receiving filters
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      038e58a2: ndt_2c Msg: Start receiving
      038e58a2: ndt_2c Msg: Sending 300 packets with size 128 bytes to Multicast Addr
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Instance 0 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 1 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 2 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 3 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 4 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 5 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 6 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 7 received expected 300 packets
      038e58a2: ndt_2c Msg: Setting receiving filters
      038e58a2: ndt_2c Msg: Set filter FILTER_NONE for instance 0
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+ for instance 1
      038e58a2: ndt_2c Msg: Set filter FILTER_BROADCAST+ for instance 2
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+ for instance 3
      038e58a2: ndt_2c Msg: Set filter FILTER_PROMISCUOUS+ for instance 4
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_PROMISCUOUS+ for instance 5
      038e58a2: ndt_2c Msg: Set filter FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      038e58a2: ndt_2c Msg: Start receiving
      038e58a2: ndt_2c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Instance 0 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 1 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 2 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 3 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 4 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 5 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 6 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 7 received expected 300 packets
      038e58a2: ndt_2c Msg: Setting receiving filters
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+ for instance 0
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+ for instance 1
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+ for instance 2
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+ for instance 3
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      038e58a2: ndt_2c Msg: Start receiving
      038e58a2: ndt_2c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Instance 0 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 1 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 2 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 3 properly didn't receive packets
      038e58a2: ndt_2c Msg: Instance 4 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 5 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 6 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 7 received expected 300 packets
      038e58a2: ndt_2c Msg: Setting receiving filters
      038e58a2: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+ for instance 0
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+ for instance 1
      038e58a2: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      038e58a2: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      038e58a2: ndt_2c Msg: Set filter FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      038e58a2: ndt_2c Msg: Start receiving
      038e58a2: ndt_2c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Instance 0 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 1 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 2 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 3 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 4 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 5 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 6 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 7 received expected 300 packets
      038e58a2: ndt_2c Msg: Setting receiving filters
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 0
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+ for instance 1
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 2
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+ for instance 3
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 4
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_PROMISCUOUS+ for instance 5
      038e58a2: ndt_2c Msg: Set filter FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 6
      038e58a2: ndt_2c Msg: Set filter FILTER_DIRECTED+FILTER_MULTICAST+FILTER_ALL_MULTICAST+FILTER_BROADCAST+FILTER_PROMISCUOUS+ for instance 7
      038e58a2: ndt_2c Msg: Start receiving
      038e58a2: ndt_2c Msg: Sending 300 packets with size 128 bytes to Bad Multicast Addr
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Instance 0 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 1 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 2 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 3 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 4 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 5 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 6 received expected 300 packets
      038e58a2: ndt_2c Msg: Instance 7 received expected 300 packets
      038e58a2: ndt_2c Msg: Unbinding adapters
   END TEST: "2c_FilterReceive", PASSED, Time=291.392
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      2c_FilterReceive
*** Test ID:        3
*** Library Path:   \ndt_2c.dll
*** Command Line:   -t AX88772b1 -s AX88772b1
*** Result:         Passed
*** Random Seed:    25237
*** Thread Count:   1
*** Execution Time: 0:04:51.392
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=4>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      2c_MulticastReceive
*** Test ID:        4
*** Library Path:   \ndt_2c.dll
*** Command Line:   -t AX88772b1 -s AX88772b1
*** Random Seed:    16916
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "2c_MulticastReceive", Threads=0, Seed=16916
      038e58a2: ndt_2c Msg: Start 1c_MulticastReceive test
      038e58a2: ndt_2c Msg: The test adapter is AX88772b1
      038e58a2: ndt_2c Msg: The support adapter is AX88772b1
      038e58a2: ndt_2c Msg: Opening adapters
      038e58a2: ndt_2c Msg: Binding adapters
      038e58a2: ndt_2c Msg: Get basic adapters info
      038e58a2: ndt_2c Msg: Add multicast addresses
      038e58a2: ndt_2c Msg: Set multicast filter
      038e58a2: ndt_2c Msg: Sending 10 packets on 8 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 80 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 64 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 640 packets
      038e58a2: ndt_2c Msg: Removing randomly 8 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 16 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 160 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 56 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 560 packets
      038e58a2: ndt_2c Msg: Removing randomly 8 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 24 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 240 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 48 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 480 packets
      038e58a2: ndt_2c Msg: Removing randomly 8 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 32 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 320 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 40 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 400 packets
      038e58a2: ndt_2c Msg: Removing randomly 8 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 40 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 400 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 32 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 320 packets
      038e58a2: ndt_2c Msg: Removing randomly 4 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 44 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 440 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 28 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 280 packets
      038e58a2: ndt_2c Msg: Removing randomly 4 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 48 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 480 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 24 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 240 packets
      038e58a2: ndt_2c Msg: Removing randomly 4 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 52 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 520 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 20 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 200 packets
      038e58a2: ndt_2c Msg: Removing randomly 4 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 56 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 560 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 16 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 160 packets
      038e58a2: ndt_2c Msg: Removing randomly 1 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 57 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 570 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 15 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 150 packets
      038e58a2: ndt_2c Msg: Removing randomly 1 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 58 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 580 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 14 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 140 packets
      038e58a2: ndt_2c Msg: Removing randomly 1 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 59 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 590 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 13 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 130 packets
      038e58a2: ndt_2c Msg: Removing randomly 1 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 60 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 600 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 12 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 120 packets
      038e58a2: ndt_2c Msg: Removing randomly 1 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 61 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 610 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 11 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 110 packets
      038e58a2: ndt_2c Msg: Removing randomly 1 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 62 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 620 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 10 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 100 packets
      038e58a2: ndt_2c Msg: Removing randomly 1 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 63 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 630 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 9 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 90 packets
      038e58a2: ndt_2c Msg: Removing randomly 1 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 64 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 640 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 8 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 80 packets
      038e58a2: ndt_2c Msg: Removing randomly 1 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 65 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 650 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 7 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 70 packets
      038e58a2: ndt_2c Msg: Removing randomly 1 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 66 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 660 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 6 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 60 packets
      038e58a2: ndt_2c Msg: Removing randomly 1 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 67 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 670 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 5 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 50 packets
      038e58a2: ndt_2c Msg: Removing randomly 1 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 68 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 680 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 4 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 40 packets
      038e58a2: ndt_2c Msg: Removing randomly 1 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 69 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 690 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 3 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 30 packets
      038e58a2: ndt_2c Msg: Removing randomly 1 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 70 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 700 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 2 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 20 packets
      038e58a2: ndt_2c Msg: Removing randomly 1 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 71 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 710 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Sending 10 packets on 1 multicast addresses
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly received 10 packets
      038e58a2: ndt_2c Msg: Removing randomly 1 multicast addresses
      038e58a2: ndt_2c Msg: Sending 10 packets on 72 unused multicast addresses
      038e58a2: ndt_2c Msg: Sent 720 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Properly didn't receive packets
      038e58a2: ndt_2c Msg: Closing adapters
   END TEST: "2c_MulticastReceive", PASSED, Time=222.559
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      2c_MulticastReceive
*** Test ID:        4
*** Library Path:   \ndt_2c.dll
*** Command Line:   -t AX88772b1 -s AX88772b1
*** Result:         Passed
*** Random Seed:    16916
*** Thread Count:   1
*** Execution Time: 0:03:42.559
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=5>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      2c_StressSend
*** Test ID:        5
*** Library Path:   \ndt_2c.dll
*** Command Line:   -t AX88772b1 -s AX88772b1
*** Random Seed:    22511
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "2c_StressSend", Threads=0, Seed=22511
      038e58a2: ndt_2c Msg: Start 2c_StressSend test
      038e58a2: ndt_2c Msg: The test adapter is AX88772b1
      038e58a2: ndt_2c Msg: The support adapter is AX88772b1
      038e58a2: ndt_2c Msg: Opening adapters
      038e58a2: ndt_2c Msg: Binding adapters
      038e58a2: ndt_2c Msg: Get basic adapters info
      038e58a2: ndt_2c Msg: Seting direct receive filters
      038e58a2: ndt_2c Msg: Test Pass #0
      038e58a2: ndt_2c Msg: Start sending 10000 packets
      038e58a2: ndt_2c Msg: Sent 10000 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Test: Sent 10000 packets with total size 7789701 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Test: Recv 10000 packets with total size 460000 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Support: Recv 10000 packets with total size 7789701 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Support: Sent 10000 packets with total size 460000 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Test Pass #1
      038e58a2: ndt_2c Msg: Start sending 10000 packets
      038e58a2: ndt_2c Msg: Sent 10000 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Test: Sent 10000 packets with total size 7859208 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Test: Recv 10000 packets with total size 460000 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Support: Recv 10000 packets with total size 7859208 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Support: Sent 10000 packets with total size 460000 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Test Pass #2
      038e58a2: ndt_2c Msg: Start sending 10000 packets
      038e58a2: ndt_2c Msg: Sent 10000 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Test: Sent 10000 packets with total size 7877852 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Test: Recv 10000 packets with total size 460000 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Support: Recv 10000 packets with total size 7877852 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Support: Sent 10000 packets with total size 460000 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Test Pass #3
      038e58a2: ndt_2c Msg: Start sending 100 packets
      038e58a2: ndt_2c Msg: Sent 100 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Test: Sent 100 packets with total size 9650 bytes in 120 ms
      038e58a2: ndt_2c Msg: Test: Recv 100 packets with total size 4600 bytes in 120 ms
      038e58a2: ndt_2c Msg: Support: Recv 100 packets with total size 9650 bytes in 120 ms
      038e58a2: ndt_2c Msg: Support: Sent 100 packets with total size 4600 bytes in 120 ms
      038e58a2: ndt_2c Msg: Test Pass #4
      038e58a2: ndt_2c Msg: Start sending 53 packets
      038e58a2: ndt_2c Msg: Sent 53 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Test: Sent 53 packets with total size 3869 bytes in 60 ms
      038e58a2: ndt_2c Msg: Test: Recv 53 packets with total size 3869 bytes in 60 ms
      038e58a2: ndt_2c Msg: Support: Recv 53 packets with total size 3869 bytes in 60 ms
      038e58a2: ndt_2c Msg: Support: Sent 53 packets with total size 3869 bytes in 60 ms
      038e58a2: ndt_2c Msg: Test Pass #5
      038e58a2: ndt_2c Msg: Start sending 10000 packets
      038e58a2: ndt_2c Msg: Sent 10000 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Test: Sent 10000 packets with total size 1140000 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Test: Recv 10000 packets with total size 460000 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Support: Recv 10000 packets with total size 1140000 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Support: Sent 10000 packets with total size 460000 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Test Pass #6
      038e58a2: ndt_2c Msg: Start sending 10000 packets
      038e58a2: ndt_2c Msg: Sent 10000 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Test: Sent 10000 packets with total size 7743450 bytes in 12492 ms
      038e58a2: ndt_2c Msg: Test: Recv 10000 packets with total size 460000 bytes in 12492 ms
      038e58a2: ndt_2c Msg: Support: Recv 10000 packets with total size 7743450 bytes in 12492 ms
      038e58a2: ndt_2c Msg: Support: Sent 10000 packets with total size 460000 bytes in 12492 ms
      038e58a2: ndt_2c Msg: Test Pass #7
      038e58a2: ndt_2c Msg: Start sending 10000 packets
      038e58a2: ndt_2c Msg: Sent 10000 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Test: Sent 10000 packets with total size 7749987 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Test: Recv 10000 packets with total size 460000 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Support: Recv 10000 packets with total size 7749987 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Support: Sent 0 packets with total size 0 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Test Pass #8
      038e58a2: ndt_2c Msg: Start sending 10000 packets
      038e58a2: ndt_2c Msg: Sent 10000 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Test: Sent 10000 packets with total size 7763422 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Test: Recv 10000 packets with total size 7763422 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Support: Recv 10000 packets with total size 7763422 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Support: Sent 10000 packets with total size 7763422 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Test Pass #9
      038e58a2: ndt_2c Msg: Start sending 10000 packets
      038e58a2: ndt_2c Msg: Sent 10000 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Test: Sent 10000 packets with total size 740000 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Test: Recv 10000 packets with total size 740000 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Support: Recv 10000 packets with total size 740000 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Support: Sent 10000 packets with total size 740000 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Unbinding adapters
      038e58a2: ndt_2c Msg: Closing adapters
   END TEST: "2c_StressSend", PASSED, Time=122.812
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      2c_StressSend
*** Test ID:        5
*** Library Path:   \ndt_2c.dll
*** Command Line:   -t AX88772b1 -s AX88772b1
*** Result:         Passed
*** Random Seed:    22511
*** Thread Count:   1
*** Execution Time: 0:02:02.812
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
<TESTCASE ID=6>
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
*** TEST STARTING
***
*** Test Name:      2c_StressReceive
*** Test ID:        6
*** Library Path:   \ndt_2c.dll
*** Command Line:   -t AX88772b1 -s AX88772b1
*** Random Seed:    8014
*** Thread Count:   0
*** vvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvvv
   BEGIN TEST: "2c_StressReceive", Threads=0, Seed=8014
      038e58a2: ndt_2c Msg: Start 2c_StessReceive test
      038e58a2: ndt_2c Msg: The test adapter is AX88772b1
      038e58a2: ndt_2c Msg: The support adapter is AX88772b1
      038e58a2: ndt_2c Msg: Opening adapters
      038e58a2: ndt_2c Msg: Binding adapters
      038e58a2: ndt_2c Msg: Get basic adapters info
      038e58a2: ndt_2c Msg: Seting direct receive filters
      038e58a2: ndt_2c Msg: Test Pass #0
      038e58a2: ndt_2c Msg: Start sending 10000 packets
      038e58a2: ndt_2c Msg: Sent 10000 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Support: Sent 10000 packets with total size 7784849 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Support: Recv 10000 packets with total size 460000 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Test: Recv 10000 packets with total size 7784849 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Test: Sent 10000 packets with total size 460000 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Test Pass #1
      038e58a2: ndt_2c Msg: Start sending 10000 packets
      038e58a2: ndt_2c Msg: Sent 10000 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Support: Sent 10000 packets with total size 7827513 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Support: Recv 10000 packets with total size 460000 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Test: Recv 10000 packets with total size 7827513 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Test: Sent 10000 packets with total size 460000 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Test Pass #2
      038e58a2: ndt_2c Msg: Start sending 10000 packets
      038e58a2: ndt_2c Msg: Sent 10000 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Support: Sent 10000 packets with total size 7714169 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Support: Recv 10000 packets with total size 460000 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Test: Recv 10000 packets with total size 7714169 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Test: Sent 10000 packets with total size 460000 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Test Pass #3
      038e58a2: ndt_2c Msg: Start sending 100 packets
      038e58a2: ndt_2c Msg: Sent 100 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Support: Sent 100 packets with total size 9650 bytes in 120 ms
      038e58a2: ndt_2c Msg: Support: Recv 100 packets with total size 4600 bytes in 120 ms
      038e58a2: ndt_2c Msg: Test: Recv 100 packets with total size 9650 bytes in 120 ms
      038e58a2: ndt_2c Msg: Test: Sent 100 packets with total size 4600 bytes in 120 ms
      038e58a2: ndt_2c Msg: Test Pass #4
      038e58a2: ndt_2c Msg: Start sending 53 packets
      038e58a2: ndt_2c Msg: Sent 53 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Support: Sent 53 packets with total size 3869 bytes in 60 ms
      038e58a2: ndt_2c Msg: Support: Recv 53 packets with total size 3869 bytes in 60 ms
      038e58a2: ndt_2c Msg: Test: Recv 53 packets with total size 3869 bytes in 60 ms
      038e58a2: ndt_2c Msg: Test: Sent 53 packets with total size 3869 bytes in 60 ms
      038e58a2: ndt_2c Msg: Test Pass #5
      038e58a2: ndt_2c Msg: Start sending 10000 packets
      038e58a2: ndt_2c Msg: Sent 10000 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Support: Sent 10000 packets with total size 1140000 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Support: Recv 10000 packets with total size 460000 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Test: Recv 10000 packets with total size 1140000 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Test: Sent 10000 packets with total size 460000 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Test Pass #6
      038e58a2: ndt_2c Msg: Start sending 10000 packets
      038e58a2: ndt_2c Msg: Sent 10000 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Support: Sent 10000 packets with total size 7840450 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Support: Recv 10000 packets with total size 460000 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Test: Recv 10000 packets with total size 7840450 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Test: Sent 10000 packets with total size 460000 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Test Pass #7
      038e58a2: ndt_2c Msg: Start sending 10000 packets
      038e58a2: ndt_2c Msg: Sent 10000 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Support: Sent 10000 packets with total size 7826097 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Support: Recv 10000 packets with total size 460000 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Test: Recv 10000 packets with total size 7826097 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Test: Sent 0 packets with total size 0 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Test Pass #8
      038e58a2: ndt_2c Msg: Start sending 10000 packets
      038e58a2: ndt_2c Msg: Sent 10000 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Support: Sent 10000 packets with total size 7736027 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Support: Recv 10000 packets with total size 7736027 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Test: Recv 10000 packets with total size 7736027 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Test: Sent 10000 packets with total size 7736027 bytes in 12490 ms
      038e58a2: ndt_2c Msg: Test Pass #9
      038e58a2: ndt_2c Msg: Start sending 10000 packets
      038e58a2: ndt_2c Msg: Sent 10000 packets
      038e58a2: ndt_2c Msg: Stop receiving and checking results
      038e58a2: ndt_2c Msg: Support: Sent 10000 packets with total size 740000 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Support: Recv 10000 packets with total size 740000 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Test: Recv 10000 packets with total size 740000 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Test: Sent 10000 packets with total size 740000 bytes in 12491 ms
      038e58a2: ndt_2c Msg: Unbinding adapters
      038e58a2: ndt_2c Msg: Closing adapters
   END TEST: "2c_StressReceive", PASSED, Time=122.813
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
*** TEST COMPLETED
***
*** Test Name:      2c_StressReceive
*** Test ID:        6
*** Library Path:   \ndt_2c.dll
*** Command Line:   -t AX88772b1 -s AX88772b1
*** Result:         Passed
*** Random Seed:    8014
*** Thread Count:   1
*** Execution Time: 0:02:02.813
*** ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

</TESTCASE RESULT="PASSED">
END GROUP: ndt_2c.dll
*** ==================================================================
*** MEMORY INFO
***
*** Memory Total:    24,485,888 bytes
*** Memory Used:     10,903,552 bytes
*** Memory Free:     13,582,336 bytes
***
*** Kernel Used:        933,888 bytes
*** Water Mark:           3,283 pages
***
*** Store Total:     24,416,256 bytes
*** Store Used:         619,860 bytes
*** Store Free:      23,796,396 bytes
*** ==================================================================

*** ==================================================================
*** SUITE SUMMARY
***
*** Passed:          6
*** Failed:          0
*** Skipped:         0
*** Aborted:         0
*** -------- ---------
*** Total:           6
***
*** Cumulative Test Execution Time: 0:19:01.234
*** Total Tux Suite Execution Time: 0:19:02.892
*** CPU Idle Time:                  0:18:41.193
*** ==================================================================
</TESTGROUP>
@@@@@@0

